{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["360QexF","汇总"],"not_rendered":{"images":1,"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"360QexF","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"汇总","index":1,"n_rows":63,"n_cols":8,"rows_kept":63,"merged":[[0,0,0,7],[1,0,1,7],[3,0,3,7],[39,0,39,7]],"flags":["formulas_cached_only"]}
[]
["项目名称：铜陵有色集团研发基地配电柜箱项目"]
["序号","名称  ","型号规格","单位","数量",null,null,"备注"]
["检测楼"]
[1,"一层楼层配电柜","XL21:800*400*2000","台",1,null,null,"1AC"]
[2,"二层楼层配电柜","XL21:800*400*2000","台",1,null,null,"2AC"]
[3,"三层楼层配电柜","XL21:800*400*2000","台",1,null,null,"3AC"]
[4,"四层楼层配电柜","XL21:800*400*2000","台",1,null,null,"4AC"]
[5,"环保设备配电柜","户外304不锈钢XL21:800*400*1800","台",1,null,null,"AH"]
[6,"组合空调配电柜","户外304不锈钢XL21:800*400*1800","台",1,null,null,"AM"]
[7,"大型实验室末端配电箱","JXF:800*600*200","台",3,null,null,"AP1-AP3"]
[8,"中型实验室末端配电箱","JXF:500*600*200","台",4,null,null,"1AZ1.3AZ1~3"]
[9,"办公室及小型实验室末端配电箱","PZ30-20(暗装)","台",74,null,null,"1AX1~20,2AX1~16,3AX1~21,4AX1~17"]
[10,"开水器终端箱","PZ30-8(暗装)","台",4,null,null,"1AK-4AK"]
[11,"楼层公共走道照明配电箱","PZ30-8(暗装)","台",4,null,null,"1AL-4AL"]
[12,"研究所双电源分置柜","XL21:800*400*2000","台",1,null,null,"AF"]
[13,"电梯机房配电箱","JXF:800*600*200","台",1,null,null,"AJ1"]
[14,"网络机房配电箱","JXF:800*600*200","台",1,null,null,"AJ2"]
[15,"一层排烟机房配电箱","304不锈钢户外:800*600*200","台",1,null,null,"AT1"]
[16,"一层消防控制室配电箱","JXF:800*600*200","台",1,null,null,"AT3"]
[17,"屋面排烟机房配电箱","304不锈钢户外:800*600*200","台",1,null,null,"AT2"]
[18,"一层楼层配电柜","XL21:800*400*2000","台",1,null,null,"1BC"]
[19,"二层楼层配电柜","XL21:800*400*2000","台",1,null,null,"2BC"]
[20,"三层楼层配电柜","XL21:800*400*2000","台",1,null,null,"3BC"]
[21,"四层楼层配电柜","XL21:800*400*2000","台",1,null,null,"4BC"]
[22,"环保设备配电柜","户外304不锈钢XL21:800*400*1800","台",1,null,null,"BH"]
[23,"组合空调配电柜","户外304不锈钢XL21:800*400*1800","台",1,null,null,"BM"]
[24,"大型实验室末端配电箱","XL21:800*400*2000","台",2,null,null,"BP1-BP2"]
[25,"中型实验室末端配电箱","JXF:500*600*200","台",9,null,null,"1BZ1~4,2BZ1~2,3BZ1,4BZ1~2"]
[26,"办公室及小型实验室末端配电箱","PZ30-20(暗装)","台",56,null,null,"1BX1~20,2BX1~10,3BX1~13,4BX1~13"]
[27,"开水器终端箱","PZ30-8(暗装)","台",4,null,null,"1BK-4BK"]
[28,"楼层公共走道照明配电箱","PZ30-8(暗装)","台",4,null,null,"1BL-4BL"]
[29,"电热板实验室末端配电箱","PZ30-20(明装)","台",15,null,null,"1BR1~2,2BR1~4,3BR1~5,4BR1~4"]
[30,"二层光谱室配电箱","PZ30-20(明装)","台",4,null,null,"2BG1~4"]
[31,"检测楼双电源分置柜","XL21:800*400*2000","台",1,null,null,"AF"]
[32,"屋面排烟机房配电箱","304不锈钢户外:800*600*200","台",2,null,null,"BT1.2"]
[33,"电梯机房配电箱","JXF:800*600*200","台",1,null,null,"BJ1"]
[34,"各房间轴流风机控制箱","JXF:200*300*200","台",40,null,null,"轴流风机控制箱"]
[35,"A型应急照明集中电源电源","JXF:800*600*200","台",1,null,null,"ALE"]
["扩大实验室"]
[36,"低压柜","GGD:800*600*2200","台",1,null,null,"AN1"]
[37,"低压柜","GGD:800*600*2200","台",1,null,null,"AN2"]
[38,"低压柜","GGD:800*600*2200","台",1,null,null,"AN3"]
[39,"照明配电箱","PZ30-20(明装)","台",1,null,null,"AL1"]
[40,"照明配电箱","PZ30-20(明装)","台",1,null,null,"AL2"]
[41,"照明配电箱","PZ30-18(明装)","台",1,null,null,"AL3"]
[42,"照明配电箱","PZ30-10(明装)","台",1,null,null,"AL4"]
[43,"照明配电箱","PZ30-10(明装)","台",1,null,null,"AL5"]
[44,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD1-FZX"]
[45,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD2-FZX"]
[46,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD3-FZX"]
[47,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD4-FZX"]
[48,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD5-FZX"]
[49,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD6-FZX"]
[50,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD7-FZX"]
[51,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD8-FZX"]
[52,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD9-FZX"]
[53,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD10-FZX"]
[54,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD11-FZX"]
[55,"防腐混合动力配电箱","304不锈钢800*600*200","台",1,null,null,"AD12-FZX"]
[56,"终端配电箱","JXF:800*600*200","台",1,null,null,"AP1(综合仓库)"]
[57,"路灯照明控制箱","JXF:800*600*200","台",1,null,null,"DL(室外路灯)"]
["合计",null,null,"台",268]